| Australian Digital Health Agency FHIR Implementation Guide 1.0.0

Australian Digital Health Agency FHIR Implementation Guide. This is the current published version. It is based on FHIR® version 4.0.1. See the Directory of published versions for a list of available versions.

#### StructureDefinition: ADHADeviceSystem - Mappings

Mappings for the dh-device-system-1 Profile.

### Mappings for RIM Mapping (http://hl7.org/v3)

ADHADeviceSystem
Device | Entity. Role, or Act, Device
text | Act.text?
contained | N/A
extension | N/A
modifierExtension | N/A
identifier | .id
identifier (paid) | n/a, II - The Identifier class is a little looser than the v3 type II because it allows URIs as well as registered OIDs or GUIDs. Also maps to Role[classCode=IDENT]
udiCarrier | .id and .code
id | n/a
extension | n/a
modifierExtension | N/A
deviceIdentifier | Role.id.extension
issuer | Role.id.root
jurisdiction | Role.scoper
carrierAIDC | Role.id.extension
carrierHRF | Role.id.extension
entryType | NA
status | .statusCode
distinctIdentifier | .lotNumberText
manufacturer | .playedRole[typeCode=MANU].scoper.name
manufactureDate | .existenceTime.low
expirationDate | .expirationTime
lotNumber | .lotNumberText
serialNumber | .playedRole[typeCode=MANU].id
deviceName |
id | n/a
extension | n/a
modifierExtension | N/A
type | .playedRole[typeCode=MANU].code
modelNumber | .softwareName (included as part)
partNumber | .playedRole[typeCode=MANU].id
specialization |
id | n/a
extension | n/a
modifierExtension | N/A
version |
id | n/a
extension | n/a
modifierExtension | N/A
property |
id | n/a
extension | n/a
modifierExtension | N/A
patient | .playedRole[typeCode=USED].scoper.playedRole[typeCode=PAT]
owner | .playedRole[typeCode=OWN].scoper
contact | .scopedRole[typeCode=CON].player
location | .playedRole[typeCode=LOCE].scoper
url | .telecom
note | .text
safety | NA

### Mappings for FiveWs Pattern Mapping (http://hl7.org/fhir/fivews)

ADHADeviceSystem
Device |
identifier | FiveWs.identifier
udiCarrier | FiveWs.identifier
deviceIdentifier | FiveWs.what[x]
status | FiveWs.status
statusReason | FiveWs.status
distinctIdentifier | FiveWs.what[x]
manufacturer | FiveWs.what[x]
manufactureDate | FiveWs.what[x]
expirationDate | FiveWs.what[x]
lotNumber | FiveWs.what[x]
serialNumber | FiveWs.what[x]
deviceName |
type | FiveWs.what[x]
modelNumber | FiveWs.what[x]
partNumber | FiveWs.what[x]
specialization |
version | FiveWs.what[x]
version |
component | FiveWs.what[x]
patient | FiveWs.subject[x], FiveWs.subject
owner | FiveWs.source
contact | FiveWs.source
location | FiveWs.where[x]
url | FiveWs.where[x]

### Mappings for UDI Mapping (http://fda.gov/UDI)

ADHADeviceSystem
Device |
identifier | The serial number which is a component of the production identifier (PI), a conditional, variable portion of a UDI. The identifier.type code should be set to “SNO”(Serial Number) and the system left empty.
udiCarrier |
deviceIdentifier | The device identifier (DI), a mandatory, fixed portion of a UDI that identifies the labeler and the specific version or model of a device.
issuer | All UDIs are to be issued under a system operated by an Jurisdiction-accredited issuing agency. GS1 DIs: http://hl7.org/fhir/NamingSystem/gs1 HIBCC DIs: http://hl7.org/fhir/NamingSystem/hibcc ICCBBA DIs for blood containers: http://hl7.org/fhir/NamingSystem/iccbba-blood ICCBA DIs for other devices: http://hl7.org/fhir/NamingSystem/iccbba-other
carrierAIDC | A unique device identifier (UDI) on a device label a form that uses automatic identification and data capture (AIDC) technology.
carrierHRF | A unique device identifier (UDI) on a device label in plain text
distinctIdentifier | The lot or batch number within which a device was manufactured - which is a component of the production identifier (PI), a conditional, variable portion of a UDI.
manufacturer | N/A
manufactureDate | The date a specific device was manufactured - which is a component of the production identifier (PI), a conditional, variable portion of a UDI. For FHIR, The datetime syntax must converted to YYYY-MM-DD[THH:MM:SS]. If hour is present, the minutes and seconds should both be set to “00”.
expirationDate | the expiration date of a specific device - which is a component of the production identifier (PI), a conditional, variable portion of a UDI. For FHIR, The datetime syntax must converted to YYYY-MM-DD[THH:MM:SS]. If hour is present, the minutes and seconds should both be set to “00”.
lotNumber | The lot or batch number within which a device was manufactured - which is a component of the production identifier (PI), a conditional, variable portion of a UDI.