Provider Connect Australia (PCA)
24.2.0.0 - active

Provider Connect Australia (PCA) - Local Development build (v24.2.0.0) built by the FHIR (HL7® FHIR® Standard) Build Tools. See the Directory of published versions

## Resource Profile: PcaLocation - Mappings

Active as of 2024-09-23

Mappings for the pca-location resource profile.

### Mappings for RIM Mapping (http://hl7.org/v3)

PcaLocation
Location | Entity. Role, or Act, .Role[classCode=SDLC]
text | Act.text?
contained | N/A
modifierExtension | N/A
identifier | n/a, II - The Identifier class is a little looser than the v3 type II because it allows URIs as well as registered OIDs or GUIDs. Also maps to Role[classCode=IDENT]
identifier (pca-li) | n/a, II - The Identifier class is a little looser than the v3 type II because it allows URIs as well as registered OIDs or GUIDs. Also maps to Role[classCode=IDENT]
status | .statusCode
operationalStatus | n/a
name | .name
alias | .name
description | .playingEntity[classCode=PLC determinerCode=INSTANCE].desc
mode | .playingEntity[classCode=PLC].determinerCode
type | .code
telecom | .telecom
address | n/a, AD
physicalType | .playingEntity [classCode=PLC].code
position | .playingEntity [classCode=PLC determinerCode=INSTANCE].positionText
id | n/a
extension | n/a
modifierExtension | N/A
longitude | (RIM Opted not to map the sub-elements of GPS location, is now an OBS)
latitude | (RIM Opted not to map the sub-elements of GPS location, is now an OBS)
altitude | (RIM Opted not to map the sub-elements of GPS location, is now an OBS)
managingOrganization | .scopingEntity[classCode=ORG determinerKind=INSTANCE]
partOf | .inboundLink[typeCode=PART].source[classCode=SDLC]
hoursOfOperation | .effectiveTime
id | n/a
extension | n/a
modifierExtension | N/A
daysOfWeek | .effectiveTime
allDay | .effectiveTime
openingTime | .effectiveTime
closingTime | .effectiveTime
availabilityExceptions | n/a
endpoint | n/a

### Mappings for FiveWs Pattern Mapping (http://hl7.org/fhir/fivews)

PcaLocation
Location |
status | FiveWs.status
operationalStatus | FiveWs.status
mode | FiveWs.class
type | FiveWs.class
physicalType | FiveWs.class